
# Device Component Details Ethernet Details

## Structure

`DeviceComponentDetailsEthernetDetails`

## Fields

| Name | Type | Tags | Description | Getter | Setter |
|  --- | --- | --- | --- | --- | --- |
| `active` | `?bool` | Optional | A boolean to represent whether the Ethernet interface is currently active. | getActive(): ?bool | setActive(?bool active): void |
| `ipAddressV4` | `?string` | Optional | The string representation of the device’s IPv4 address. | getIpAddressV4(): ?string | setIpAddressV4(?string ipAddressV4): void |

## Example (as JSON)

```json
{
  "active": false,
  "ip_address_v4": "ip_address_v46"
}
```

